**YNZ Daily Vessel Check Sheet**

**Version 2**

**December 2017**

**Boat check Done**

|  |  |
| --- | --- |
| Hull sound (Tubes properly inflated if fitted) |  |
| Bungs in place |  |
| Oil level checked (or premixed with fuel) |  |
| Fuel on board and tank full |  |
| Battery charged (if fitted) |  |
| Kill cord on engine |  |
| Anchor bitter end secured to vessel |  |

**Safety Equipment On Board**

|  |  |
| --- | --- |
| Personal Floatation Devices on board (one for each crew) |  |
| VHF radio (battery charged) |  |
| Knife |  |
| Towing line |  |
| Bailer |  |
| Anchor |  |
| Alternative means of propulsion (i.e. Oars) |  |
| First Aid Kit |  |

\* - add more as required